# SAP Application User Guide

### Preparing the phone for a Sim Access Profile connection

1. Bluetooth is enabled on the mobile phone. The ‘Turn on Bluetooth’ checkbox under
   Settings-Bluetooth is checked.
2. If this is the first time you are attempting to connect to the phone from the carkit,
   ensure that the ‘Make this device discoverable to other devices’ checkbox is checked.
3. Ensure that the ‘Remote SIM Access’ checkbox in the application window is checked
4. To enable downloading ‘Contacts’ from the phone SIM onto the carkit, ensure that all
   your ‘Contacts’ on the phone are stored in the SIM card and not in Phone Memory.
   Configure the carkit to download Contacts only from SIM Memory. Note that any other
   setting can lead to an error during Contacts Download.

Enabling remote access to the phone's Sim

1. Remote SIM Access’ checkbox should be checked, then Sim Access Profile server is running and will accept connections from clients.
2. These clients can access the phone’s SIM card.

Disabling remote access to the phone's Sim

1. Remote SIM Access’ checkbox is unchecked, the Sim Access Profile will refuse incoming connection requests.
2. In this mode, clients cannot connect to or access the phone’s SIM card.

Connecting to the Pocket PC from the Car kit

1. Search for Bluetooth Devices on the Carkit.
2. If your Pocket PC is set to Discoverable , it will show up on the Carkit LCD as a possible server.
3. Choose to connect to your PocketPC from the carkit.
4. If this is the first time you are pairing the Carkit with the PocketPC, you’ll be required to enter the 16-digit pin key displayed on the Carkit LCD into the PocketPC. Do so.
5. You’ll then see a pop up ‘Remote connection established with <client>’.
6. In the case of the Nokia 610 Carkit, the pop will say ‘Remote connection established with Nokia 610’.
7. Select OK in the pop up
8. Select Done in the screen that informs you that a connection with the Carkit has been established.

### Using the Sim Access Profile connection

1. After a Sim Access Profile connection is established between the PocketPC and the Carkit, you will no longer be able to use the phone for telephony.
2. Navigate to a particular contact or enter the phone number you wish to call on the Carkit
3. Make the call.You will be able to perform all telephony related activities (making and receiving calls,
   sending and receiving messages, browsing contacts, call registers etc.) on the Carkit until the SAP connection is active.

### Disconnection initiated from the phone

1. On the Home screen, press the Start soft key.
2. Select Start -> File Explorer-> Windows --> SAPSettings.
3. You should see the following screen.
4. Select the Disconnect option on the menu bar to initiate a disconnection.
5. Select Yes in the Confirm screen that pops up.
6. After disconnection you will see the following message box. Note that disconnection may take a while, especially if it is initiated when the Carkit is engaged in a call
7. Select OK.. The SAP connection has been disconnected.

### Disconnection initiated from the Carkit

The Carkit may provide an option to disconnect from an established Sim Access Profile
connection. Even if it doesn’t, choose to switch off the Carkit. This will automatically
disconnect the connection.

1. Use the relevant option on the Carkit to disconnect from the phone. The user manual of the Carkit will contain details on how to do this.
2. You will be notified of the disconnection by the following message box on the phone.
3. Select OK. The SAP connection is disconnected.