; ea244wmi.inf
; Setup information file for NEC MultiSync EA244WMi Monitor
;
; Copyright 2015, NEC Display Solutions, Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=ea244wmi.cat
DriverVer=09/04/2015,1.15.0904.1738

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC68D4
ExcludeFromSelect.nt=Monitor\NEC68D5
ExcludeFromSelect.nt=Monitor\NEC68D6
ExcludeFromSelect.nt=Monitor\NEC68D7

[DestinationDirs]
EA244WMi.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
ea244wmi.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%EA244WMi-A%=EA244WMi-A.Install, Monitor\NEC68D4
%EA244WMi-D%=EA244WMi-D.Install, Monitor\NEC68D5
%EA244WMi-DP%=EA244WMi-DP.Install, Monitor\NEC68D6
%EA244WMi-H%=EA244WMi-H.Install, Monitor\NEC68D7

[NECDS.ntamd64]
%EA244WMi-A%=EA244WMi-A.Install.ntamd64, Monitor\NEC68D4
%EA244WMi-D%=EA244WMi-D.Install.ntamd64, Monitor\NEC68D5
%EA244WMi-DP%=EA244WMi-DP.Install.ntamd64, Monitor\NEC68D6
%EA244WMi-H%=EA244WMi-H.Install.ntamd64, Monitor\NEC68D7

[EA244WMi-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-A.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-D.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-DP.Install]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-DP.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-H.Install]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-H.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-A.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-A.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-D.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-D.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-DP.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-DP.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi-H.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=EA244WMi-H.AddReg, 1920, DPMS
CopyFiles=EA244WMi.CopyFiles

[EA244WMi.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[EA244WMi.Install.ntamd64.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1920]
HKR,,MaxResolution,,"1920,1200"

[DPMS]
HKR,,DPMS,,1

[EA244WMi-A.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30.0-77.0,55.0-61.0,+,+"
HKR,,ICMProfile,0,"ea244wmi.icm"

[EA244WMi-D.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30.0-77.0,55.0-61.0,+,+"
HKR,,ICMProfile,0,"ea244wmi.icm"

[EA244WMi-DP.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30.0-77.0,55.0-61.0,+,+"
HKR,,ICMProfile,0,"ea244wmi.icm"

[EA244WMi-H.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30.0-77.0,55.0-61.0,+,+"
HKR,,ICMProfile,0,"ea244wmi.icm"


[EA244WMi.CopyFiles]
ea244wmi.icm

[Strings]
NECDS="NEC"
Disk1="NEC Display Solutions Installation Disk"

SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

EA244WMi-A="NEC MultiSync EA244WMi(Analog)"
EA244WMi-D="NEC MultiSync EA244WMi(Digital)"
EA244WMi-DP="NEC MultiSync EA244WMi(DisplayPort)"
EA244WMi-H="NEC MultiSync EA244WMi(HDMI)"