System startup


U-Boot 2010.06-svn (Oct 21 2016 - 11:21:29)

Check Flash Memory Controller v100 ... Found
SPI Nor(cs 0) ID: 0xc2 0x20 0x17
Block:64KB Chip:8MB Name:"MX25L6406E"
SPI Nor total size: 8MB
In:    serial
Out:   serial
Err:   serial
Press Ctrl+C to stop autoboot
xmtech # printenv
bootcmd=setenv setargs setenv bootargs ${bootargs};run setargs;fload;bootm 0x82000000
bootdelay=1
baudrate=115200
bootfile="uImage"
da=mw.b 0x82000000 ff 1000000;tftp 0x82000000 u-boot.bin.img;sf probe 0;flwrite
du=mw.b 0x82000000 ff 1000000;tftp 0x82000000 user-x.cramfs.img;sf probe 0;flwrite
dr=mw.b 0x82000000 ff 1000000;tftp 0x82000000 romfs-x.cramfs.img;sf probe 0;flwrite
dw=mw.b 0x82000000 ff 1000000;tftp 0x82000000 web-x.cramfs.img;sf probe 0;flwrite
dl=mw.b 0x82000000 ff 1000000;tftp 0x82000000 logo-x.cramfs.img;sf probe 0;flwrite
dc=mw.b 0x82000000 ff 1000000;tftp 0x82000000 custom-x.cramfs.img;sf probe 0;flwrite
up=mw.b 0x82000000 ff 1000000;tftp 0x82000000 update.img;sf probe 0;flwrite
ua=mw.b 0x82000000 ff 1000000;tftp 0x82000000 upall_verify.img;sf probe 0;flwrite
tk=mw.b 0x82000000 ff 1000000;tftp 0x82000000 uImage; bootm 0x82000000
dd=mw.b 0x82000000 ff 1000000;tftp 0x82000000 mtd-x.jffs2.img;sf probe 0;flwrite
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
gatewayip=192.168.0.1
bootargs=mem=${osmem} console=ttyAMA0,115200 root=/dev/mtdblock1 rootfstype=cramfs mtdparts=hi_sfc:320K(boot),3520K(romfs),)
osmem=39M
ethaddr=00:12:16:8f:b5:df
NID=0x0003
sensortype=0x0017
appSystemLanguage=SimpChinese
appVideoStandard=PAL
stdin=serial
stdout=serial
stderr=serial
verify=n
ver=U-Boot 2010.06-svn (Oct 21 2016 - 11:21:29)

Environment size: 1407/65532 bytes
xmtech # boot
CFG_BOOT_ADDR:0x58050000
8192 KiB hi_fmc at 0:0 is now current device

### boot load complete: 1890720 bytes loaded to 0x82000000
### SAVE TO 80008000 !
## Booting kernel from Legacy Image at 82000000 ...
   Image Name:   linux
   Image Type:   ARM Linux Kernel Image (uncompressed)
   Data Size:    1890656 Bytes = 1.8 MiB
   Load Address: 80008000
   Entry Point:  80008000
   Loading Kernel Image ... OK
OK

Starting kernel ...

Uncompressing Linux... done, booting the kernel.
