SIT
MMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMMOFB
MLE
RBE
SPL Nor Load!
SPL Nor flash boot!
Secure boot enable
Secure verify ok
LzmaDecode start
LzmaDecode end(0)


U-Boot 2017.09-svn470795 (Jun 16 2022 - 15:46:36 +0800)

DRAM:  128 MiB
MMC:   dwmmc@10300000: 0
*** Warning - bad CRC, using default environment

In:    uart@0x18400000
Out:   uart@0x18400000
Err:   uart@0x18400000
Net:   eth0: ethernet@1b800000
### CRAMFS load complete: 8965 bytes loaded to 0x40000000
Hit any key to stop autoboot:  0

This program will upgrade software.
*******************************************************
*  ATTENTION!! PLEASE READ THIS NOTICE CAREFULLY!     *
*  Don't reset machine,or anything that interrupt it. *
*  The upgrade process must finish in 10 minutes!     *
*  If this program fails,machine might be unusable,   *
*  and you will need to reflash again.                *
*  If you find this too risky,power off machine now.  *
*******************************************************

Now press [u/U] key to upgrade software:b
U-Boot# setenv gateway=192.168.1.1
enter auth
CAAAALybXi9a5Yxnsek=
Password: ERROR [do_rsa_decrypt-180]:rsa_pkcs1_decrypt failed : -0x4100
ERROR [bsp_run_command-291]:Auth failed! ret=-5
U-Boot# version
enter auth
CAAAALybXi9a5RYmjKk=
Password: ERROR [bsp_run_command-291]:Auth failed! ret=-2
U-Boot# printenv
baudrate=115200
bootargs=mem=96M console=ttyS0,115200n8
bootcmd=bootm 0x40008000 0x41000000 0x41800000;
bootdelay=1
default=cramfsload 0x40008000 uImage;cramfsload 0x41000000 ramdisk.gz;cramfsload 0x41800000 common.dtb;
ethact=ethernet@1b800000
ethaddr=bc:9b:5e:2f:5a:e5
fdtcontroladdr=47f61690
filesize=2305
gatewayip=192.0.0.1
ipaddr=192.0.0.64
netmask=255.255.255.0
sec=tftp 0x40008000 uImage_sec;tftp 0x41000000 ramdisk_sec.gz;tftp 0x41800000 common_sec.dtb;bootm 0x40008000 0x41000000 0x41800000;
serverip=192.0.0.128
stderr=uart@0x18400000
stdin=uart@0x18400000
stdout=uart@0x18400000

Environment size: 626/4092 bytes
U-Boot#

