;; NETRTF.INF
;;
;; Relatek RTL8129 Fast-Ethernet Network Interface Cards.
;;
;; Copyright 1996, Realtek Semiconductor Corporation

[Version]
LayoutFile=layout.inf
Signature="$CHICAGO$"
Class=Net
Provider=%V_MS%

[Manufacturer]
%V_Realtek%=Realtek

[Realtek]
%Rtl8129.DeviceDesc%=rtl8129.ndi,PCI\VEN_10EC&DEV_8129

;[DestinationDirs]
;DefaultDestDir=11

[rtl8129.ndi]
;CopyFiles=rtl8129.CopyFiles
;DelFiles=rtl8129.DelFiles
AddReg=rtl8129.ndi.reg,rtlrtf.ndi.reg,pci129.ndi.reg

;[rtl8129.CopyFiles]
;netrtf.inf,,,2
;
;[rtl8129.DelFiles]
;drvidx.bin,,,1
;drvdata.bin,,,1

;;****************************************************************************
;;    *RTL8129   Realtek RTL8129
;;****************************************************************************

[rtl8129.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_10EC&DEV_8129"
;HKR,Ndi,DeviceID,,"*RTL8129"

HKR,Ndi\Install,,0,rtl8129.install
;HKR,NDI\Params\Speed,flag,1,30,00,00,00
;HKR,NDI\Params\EtherID,flag,1,30,00,00,00
;HKR,NDI\Params\BusNo,flag,1,30,00,00,00
;HKR,NDI\Params\DeviceNo,flag,1,30,00,00,00

;HKR,Ndi\params\Speed,ParamDesc,0,"Link Speed"
;HKR,Ndi\params\Speed,type,0,enum
;HKR,Ndi\params\Speed,default,0,auto
;HKR,Ndi\params\Speed\enum,auto,0,"Auto Detect"
;HKR,Ndi\params\Speed\enum,10,0,"10 Mb/sec"
;HKR,Ndi\params\Speed\enum,100,0,"100 Mb/sec"

;HKR,Ndi\params\EtherID,ParamDesc,0,"Ethernet ID"
;HKR,Ndi\params\EtherID,type,0,edit
;HKR,Ndi\params\EtherID,default,0,"000000000000"
;HKR,Ndi\params\EtherID,LimitText,0,12
;HKR,Ndi\params\EtherID,UpperCase,0,1
;HKR,Ndi\params\EtherID,Optional,0,1

;HKR,Ndi\params\BusNo,ParamDesc,0,"PCI Bus Number"
;HKR,Ndi\params\BusNo,type,0,int
;HKR,Ndi\params\BusNo,default,0,0
;HKR,Ndi\params\BusNo,Min,0,0
;HKR,Ndi\params\BusNo,Max,0,255
;HKR,Ndi\params\BusNo,Step,0,1
;HKR,Ndi\params\BusNo,Base,0,10
;HKR,Ndi\params\BusNo,Optional,0,1

;HKR,Ndi\params\DeviceNo,ParamDesc,0,"PCI Device Number"
;HKR,Ndi\params\DeviceNo,type,0,int
;HKR,Ndi\params\DeviceNo,default,0,0
;HKR,Ndi\params\DeviceNo,Min,0,0
;HKR,Ndi\params\DeviceNo,Max,0,31
;HKR,Ndi\params\DeviceNo,Step,0,1
;HKR,Ndi\params\DeviceNo,Base,0,10
;HKR,Ndi\params\DeviceNo,Optional,0,1



;;****************************************************************************
;;
;;****************************************************************************

[rtlrtf.ndi.reg]
; key,subkey,valuname,type,value
HKR,,DriverDesc,0,"Realtek RTL8129 PCI Fast Ethernet Controller"
HKR,,DevLoader,0,*ndis
HKR,,DeviceVxDs,0,rtl8129.sys
HKR,,EnumPropPages,0,netdi.dll,EnumPropPages

; NDIS Info
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a
HKR,NDIS,LogDriverName,0,"RTFNT"
HKR,NDIS\NDIS2,DriverName,0,"RTFND$"
HKR,NDIS\NDIS2,FileName,0,"rtfnd.dos"
HKR,NDIS\ODI,DriverName,0,"rtfodi"
HKR,NDIS\ODI,FileName,0,"rtfodi.com"

; Interfaces
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR,Ndi\Interfaces,DefUpper,0,"ndis2,ndis3"
HKR,Ndi\Interfaces,UpperRange,0,"ndis2,ndis3,odi"

; Install sections
HKR,Ndi\Install,ndis3,0,"rtlrtf.ndis3"
HKR,Ndi\Install,ndis2,0,rtlrtf.ndis2
HKR,Ndi\Install,odi,0,rtlrtf.odi

; Early Tx Threshold
HKR,Ndi\Params\EarlyTxThreshold,ParamDesc,0,"Early Tx Threshold"
HKR,Ndi\Params\EarlyTxThreshold,Type,0,"int"
HKR,Ndi\Params\EarlyTxThreshold,Default,0,"10"
HKR,Ndi\Params\EarlyTxThreshold,Flag,1,20,00,00,00
HKR,Ndi\Params\EarlyTxThreshold,Min,0,"0
HKR,Ndi\Params\EarlyTxThreshold,Max,0,"63"
HKR,Ndi\Params\EarlyTxThreshold,Step,0,"1"
HKR,Ndi\Params\EarlyTxThreshold,Base,0,"10"


HKR,NDI\Params\NetworkAddress,flag,1,30,00,00,00
HKR,Ndi\params\NetworkAddress,ParamDesc,0,"Network Address"
HKR,Ndi\params\NetworkAddress,type,0,edit
HKR,Ndi\params\NetworkAddress,default,0,"000000000000"
HKR,Ndi\params\NetworkAddress,LimitText,0,12
HKR,Ndi\params\NetworkAddress,UpperCase,0,1
HKR,Ndi\params\NetworkAddress,Optional,0,1



;;****************************************************************************
;; PCI common parameters
;;****************************************************************************

[pci129.ndi.reg]
;;params
;HKR,,MediaType,0,1
;HKR,,AdapterType,0,5
;HKR,,BusType,0,5

;; Resources
HKR,,InterruptNumber,1,04,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00
HKR,NDI\params\InterruptNumber,resc,1,04,00,00,00
HKR,Ndi\params\interruptNumber,ParamDesc,0,"Interrupt Level"
HKR,NDI\params\InterruptNumber,flag,1,20,00,00,00
HKR,NDI\params\IOBaseAddress,resc,1,02,00,00,00
HKR,NDI\params\IOBaseAddress,ParamDesc,0,"I/O Base Address"
HKR,NDI\params\IOBaseAddress,flag,1,20,00,00,00

;;ndis2
HKR,NDI\params\Interrupt,resc,1,04,00,00,00
HKR,Ndi\params\interrupt,ParamDesc,0,"Interrupt Level"
HKR,NDI\params\Interrupt,flag,1,10,00,00,00
HKR,NDI\params\IOBase,resc,1,02,00,00,00
HKR,NDI\params\IOBase,ParamDesc,0,"I/O Base Address"
HKR,NDI\params\IOBase,flag,1,10,00,00,00

;;****************************************************************************
;; Drivers
;;****************************************************************************

;; Install NDIS3
[rtlrtf.ndis3]
;CopyFiles=rtlrtf.ndis3.CopyFiles,rtl8129.inf.CopyFiles,rtl8129.help.CopyFiles
CopyFiles=rtlrtf.ndis3.CopyFiles,rtl8129.inf.CopyFiles
DelFiles=rtl8129.DelFiles

[rtlrtf.ndis3.CopyFiles]
rtl8129.sys,,,2

[rtl8129.inf.CopyFiles]
netrtf.inf,,,2

;[rtl8129.help.CopyFiles]
;rtlrtf95.txt,,,2

[rtl8129.DelFiles]
drvidx.bin,,,1
drvdata.bin,,,1

;;Install NDIS2
[rtlrtf.ndis2]
CopyFiles=rtlrtf.ndis2.CopyFiles

[rtlrtf.ndis2.CopyFiles]
rtfnd.dos,,,2

;;Install ODI
[rtlrtf.odi]
CopyFiles=ne2000.odi.CopyFiles

[rtlrtf.odi.CopyFiles]
rtfodi.com,,,2

;;****************************************************************************
;; Destination Directories
;;****************************************************************************
[DestinationDirs]
DefaultDestDir              =11 ; LDID_SYS
rtlrtf.ndis3.CopyFiles      =11
rtlrtf.ndis2.CopyFiles      =26 ; LDID_WINBOOT
rtlrtf.odi.CopyFiles        =26
rtl8129.inf.CopyFiles       =17 ; INF
rtl8129.DelFiles            =17
;rtl8129.help.CopyFiles     =?? ; Help file

[SourceDisksNames]
1="Realtek Fast Ethernet RTL8129 Adapter Driver Disk",,0

[SourceDisksFiles]
rtl8129.sys=1
netrtf.inf=1
rtfnd.dos=1
rtfodi.com=1
;rtl8129.sys=1,"win95"
;netrtf.inf=1,"win95"
;rtfnd.dos=1,"win95"
;rtfodi.com=1,"win95"

;;****************************************************************************
;; Localizable Strings
;;****************************************************************************
[strings]
;;Provider
V_MS="Microsoft"

;;Manufacturers
V_Realtek="Realtek"

;;PCI Realtek Devices
rtl8129.DeviceDesc="Realtek RTL8129 PCI Fast Ethernet"
