;
; _______________________________________________________________________
;| Monitor.INF								|
;|                                                              	|
;| This is a Setup information file for XENON monitors.			|
;|									|
;|                                          Version 3.00		|
;|                                          Dec.29.2000  		|
;|									|
;|	Copyright (C) 1998-2000 XENON Telecommunications Co., Ltd	|
;|______________________________________________________________________|
;

[version]
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
signature="$CHICAGO$"
Class=Monitor
Provider=%XENON%

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

;-------------------------------------------------
; Manufacturers

[Manufacturer]
%XENON%=XENON

;-------------------------------------------------
; Driver sections

[XENON]
%XEN-1410D1%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1410D2%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1500D%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1510D%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1510P%	= XENON_XGA.Install, Monitor\DNV0097
%VNV-1510P%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1510QE%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1510QX%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1510T%	= XENON_XGA.Install, Monitor\DNV0097
%XEN-1810E%	= XENON_SXGA.Install, Monitor\DNV00B5

;-------------------------------------------------
; Install sections

[XENON_XGA.Install]
DelReg=Del_Current_REG
AddReg=XENON_XGA.AddReg, 1024, DPMS

[XENON_SXGA.Install]
DelReg=Del_Current_REG
AddReg=XENON_SXGA.AddReg, 1280, DPMS

;-------------------------------------------------
; Common AddReg sections

[Del_Current_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[640]
HKR,,MaxResolution,,"640,480"
[800]
HKR,,MaxResolution,,"800,600"
[1024]
HKR,,MaxResolution,,"1024,768"
[1280]
HKR,,MaxResolution,,"1280,1024"
[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

;-------------------------------------------------
; Model AddReg sections

[XENON_XGA.AddReg]
HKR,"MODES\1024,768",Mode1,,"30.0-65.0,55.0-77.0,+,+"
HKR,,PreferredMode,,"1024,768,60"
HKR,,ICMProfile,1,9

[XENON_SXGA.AddReg]
HKR,"MODES\1280,1024",Mode1,,"30.0-80.0,56.0-85.0,+,+"
HKR,,PreferredMode,,"1280,1024,60"
HKR,,ICMProfile,1,9


;-------------------------------------------------
; User visible strings

[Strings]
MonitorClassName="Monitor"
XENON="XENON Telecommunications Co., Ltd"
XEN-1410D1	= "XENON  XEN-1410D1"
XEN-1410D2	= "XENON  XEN-1410D2"
XEN-1500D	= "XENON  XEN-1500D"
XEN-1510D	= "XENON  XEN-1510D"
XEN-1510P	= "XENON  XEN-1510P"
VNV-1510P	= "XENON  VNV-1510P"
XEN-1510QE	= "XENON  XEN-1510QE"
XEN-1510QX	= "XENON  XEN-1510QX"
XEN-1510T	= "XENON  XEN-1510T"
XEN-1810E	= "XENON  XEN-1810E"
